# Design and Implementation of Modified Multilevel Sepic Converter for PV Applications

T.Arunkumari, V. Indragandhi\* R.Rajasingh

*School of Electrical Engineering*

*Vellore Institute of Technology, Vellore*

*\*V. Indragandhi, arunindra08@gamil.com*

**Abstract-** **In this manuscript, a DC-DC converter of modified multilevel sepic model with single switch is proposed here. The designed converter combines the voltage tripler circuit, which improves the voltage ratio and reduces the ripple source of the scheme. Another merit of the designed converter is reduces the voltage strain and utilized for PV based applications. The functioning of the designed model in Continuous-Conduction Mode (CCM) is discussed. The converter boosts the 30 V of PV input to 400 V output voltages. The efficiency attained by the designed converter is 94%. The Theoretical examination of the designed converter is presented and it is done with MATLAB simulink. To analyse the performance of this DC-DC converter a model was developed and tested. From the investigational results obtained, it is analysed that the designed converter performs better and suitable for PV based application.**

**Keywords**: **High voltage conversion, irradiation, multilevel sepic converter, Photo Voltaic, Ripple voltage.**

I. INTRODUCTION

The changes of rising oil costs and progressively stressing level of contamination appeared differently in relation to the new arrangements of feasible improvement to make elective and sustainable power sources more alluring. Financial motivators and gigantic progression in electronic innovation advance the utilization of PV frameworks. These frameworks show a straightforward and advantageous arrangement from a financial perspective. The utilization of a converter on these photovoltaic frameworks is much additionally convincing as it builds their effectiveness and diminishes their expenses. Though, the reduced voltage level of these non-conventional energy skills requires for high efficacy heavy boost up [1]. Hypothetically, increased source level ratio could be acquired by the ordinary models, for example, voltage-lift up sort and step-up mode converters with large duty ratio [2]. Many high boosts up voltage converters are proposed to raise the voltage ratio and efficacy of the model which is categorized in to three zones [3–9].

Parallel organized arrangement of VMCs is implemented to improve the source voltage ratio limit in a stretchy path [10]. The voltage sources of all storage along the VMCs are similar through raises the elasticity of the model. An IDBS mode converter is projected as a large step-up mode power converter circuit [11]. Variant and categorization of tapping converters are represented in [12]. Parallel and stacked mode inductive coupler step up mode converters have been designed in [13-15], correspondingly. This designs converters are ease and price reasonable with only single-active control.. The authors in [16-17], ought to incorporated a waveform of a passive and a active diode hooked on the positioning the converter [20].

In [18], two ways waveform are located on together. By incorporation of HFCI and waveform in sequence mode with the switch, a easy high voltage ratio DC–DC in [19].The single switch sepic converter with VM has existed in [21].The model design in [22], involves the CI, voltage-lift technique circuit mode and the clamping mode circuit. The model in [23] is shaped by paralleling a usual boost type model and a CI boost mode by contributing the switch. This model character not only reduces ripple current, likewise quadratic- gain ratio of the converter. However, due to parallel working of this design, the efficacy is not promised.

A single active switch sort, huge step-up mode model depending on swapped model CI and switched model storage device has been accessible in [24]. Then massive input side filters must be utilized to sieve out the noise filling of input current. By the way, working, the power compactness and renovation efficacy is reduced at peak power range. In huge power applications, research analyst have been pointed on inter-leaved type mode converters owing to the merits which are propose, such as reduced input source-current, huge power compactness and huge efficacy [25-27]. On relying the above considerations, this manuscript details a novel non-isolated modified multilevel sepic converter. The PV conversion block is illustrated in Fig 1. Here the recommended converter is the combination sepic converter and voltage tripler circuit .It helps it attaining good static gain with suitable duty ratio and better efficiency. Overall, the proposed model converter full fills the following needs in PV energy transformation schemes: Higher voltage gain conversion ratio, reduced voltage strain athwart semiconductors, Recycling of inductive leakage energy, Lessening of reverse recovery diode current problems, Lessened input ripple current and high conversion rate efficacy.



Fig.1 PV energy conversion

The manuscript is prearranged as below. In section 2, the operation of the designed model in CCM is explained. In section 3 the design and examination of the projected converter is explained. In section 4 Comparative examination of projected converter with conventional model is explained. In section 5 investigational fallouts are evaluated. Conclusion is followed by section 6.

II.OPERATION OF THE PROPOSED CONVERTER

The projected circuit is represented in Fig 2. Few assumptions are made to streamline the circuit designs and operation of the projected converter.

1. The converter functions under CCM at the stable condition.
2. Semiconductor strategies are considered as ideal in nature.
3. The capacitor utilized has high storage voltage and hence the capacitors are expected to be constant. Hence the input capacitor and the output capacitor are considered as equal.

The design consists of main switch, inductors,, diodes *,,,and*  , capacitorsand output capacitor . The VT is united with basic sepic to progress the voltage improvement level of the converter. The switching limit in the semiconductor device is reduced. Capacitors operate as similar operation in conventional boost converter.



Fig.2 Proposed single switch Converter

### *2.1. Continuous conduction mode operation:*

The proposed converter functions in two manners. The modes of operations are shown in Fig.3 and Fig.4

*Mode I [t0–t1]:* When the switch is crooked-on diodes ,and is turned ON. Diode and are reverse biased. The voltage is delivered to and is delivered to. These inductors help in storing the energy. The ejects the required liveliness to the load for its operation. When the switch turns off, this mode tops. Also the diode and current attains zero at t=t1.



Fig.3. Proposed DC-DC converters turn on mode

*Mode II [t1–t2]:* When the , is bowed OFF, the diodes and are in OFF condition. The diodes and are in forward condition. The capacitors are charged by the inductor L1 and L2. The load receives the energy by discharging mode of the capacitor. This operation ends when Switch is crooked ON. The subsequent cycle continues.

The main operational waveform is represented in fig.5. The total capacitive voltage is identical to the production voltage of the model.

 **(1)**





Fig.4 Proposed DC-DC converters turn off mode



Fig. 5.CCM operation waveforms

III.ANALYSIS OF THE PROPOSED CONVERTER

Here,the theoretical analysis of the designed model is explained by following with design procedural of the converter proposed.

### *Static gain and switching voltage analysis:*

At steady condition, the inductance value is considered as null and the equation is termed as below and hence in CCM operation, the inductor L1 is given as

 (3)

Here *d* is duty cycle, input voltage is .On rearranging the values in Eq. (3), and the capacitor C0 value is obtained same as static gain..

 (4)

The inductor L2 is zero at steady state condition,

 (5)

From equation 1, capacitor 1 voltage is given by,

 (6)

By substituting the equation 3 & 4 in 5 the static gain is derived as ,

 (7)

The duty cycle equation of the converter proposed is given as,

 (8)

The capacitor voltage in C2, C3 are given as

 (9)

 (10)

The output voltage of the proposed model is given as,

 (11)

On taking the diode voltage drop in to account,

 (12)

On simplifying,

 (13)

The attained duty cycle is 0.775.

Fig.6 Converter output voltage

On comparing the proposed converter with conventional converter, the step up of voltage range is high. The comparison chart depending on output voltage is depicted in Fig.6.

IV.RESULTS AND ANALYSIS

In proposed converter output voltage ripple level is much small and the steady state is attained at earliest. The maximum over shoot is 0% and the transient response analysis is better than multilevel sepic converter. The output voltage is reliable and hence switching operation is good with reduced conduction loss and switching loss. The inductive voltage occurs only in positive value. From the fig.13, the output voltage attained from planned converter is less in ripple, the maximum over shoot is 0%, the settling period is 0.5ms and the stable state error is 0.6%. This output signifies that the converter operates in stable state. In fig. 13 current output and voltage source of projected model is depicted. There it can be noted that the current is unrestricted from disturbances and it is constant which helps the converter to be steady state manner. The output ripple is less which provides the best performance of the planned model. The parameter of the designed model is demonstrated in table 1. Hence these converter well suits for PV applications and it boost up the PV voltage to the application level.

Table 1 Proposed Converter parameters

|  |  |
| --- | --- |
| **Components** | **Parameter** |
| **Input voltage** | **30 V** |
| **Output voltage** | **400 V** |
| **Input current** | **15.2 A** |
| **Output current** | **1 A** |
| **Inductor L1, L2** | **205, 180 µH** |
| **Capacitor C1, C2, C4** | **2.2µF** |
| **Capacitor C3** | **2.2µF** |
| **Capacitor C0** | **40 µF** |
| **Resistor** | **400 Ω** |





Fig 13. simulation waveform of output voltage, output current, inductive current and capacitive voltage of proposed converter (proposed converter)

Table 2 Transient Response Analysis

|  |  |  |
| --- | --- | --- |
| **Transient response** | **Multilevel Sepic Converter** | **Proposed Converter** |
| **Settling time** | **0.5 ms** | **0.15 ms** |
| **Peak time** | **0.08 ms** | **0.03 ms** |
| **Rise time** | **0.06 ms** | **0.014 ms** |
| **Maximum overshoot** | **5%** | **0%** |
| **Steady state error** | **1.6%** | * 1. **or 0.6%** |

V.CONCLUSION

In this manuscript a step up voltage gain modified multilevel sepic converter has been proposed. The working and function of the designed circuit in model mode is elucidated. The operation of the design is detailed by the waveform depiction. The proposed model attains high static gain with reduce switching and conduction loss. The concept of VT has been embedded to improve the boosting of voltage ratio with efficiency. The steady state and design analysis has been explained. The simulation scrutiny of the projected converter is accessible clearly on comparing with multilevel sepic converter results. The transient comeback investigation of the designed model is elucidated. A model has been established in laboratory and confirmed the working of converter. The investigational results prove that the projected converter attains high stepping of voltage with tripling of voltage level with an efficiency of 94% with reduced switching stress.

**References**

1. Arunkumari, T. and Indragandhi, V.,. An overview of high voltage conversion ratio DC-DC converter configurations used in DC micro-grid architectures. *Renewable and Sustainable Energy Reviews*, Vol *77*, pp.670-687 Sep 2017.
2. Farhat, M., Barambones, O. and Sbita, L., 2017. A new maximum power point method based on a sliding mode approach for solar energy harvesting. *Applied Energy*, Vol *185*, pp.1185-1198, Jan 2017.
3. Abutbul, O., Gherlitz, A., Berkovich, Y. and Ioinovici, A., 2003. Step-up switching-mode converter with high voltage gain using a switched-capacitor circuit. *IEEE Transactions on circuits and systems I: Fundamental theory and applications*, Vol *50, no* 8, pp.1098-1102, Aug 2007.
4. Rosas-Caro, J.C., Ramirez, J.M., Peng, F.Z. and Valderrabano, A., 2010. A DC–DC multilevel boost converter. *IET Power Electronics*, Vol *3* no.1, pp.129-137, Jan 2010 .
5. Fardoun, A.A. and Ismail, E.H., 2010. Ultra step-up DC–DC converter with reduced switch stress. *IEEE transactions on industry applications*, vol *46 no* 5, pp.2025-2034 Sep 2010.
6. Nouri, T., Babaei, E. and Hosseini, S.H., 2013. A generalized ultra step-up DC–DC converter for high voltage application with design considerations. *Electric Power Systems Research*, Vol *105*, pp.71-84 Dec 13.
7. Nouri, T., Hosseini, S.H., Babaei, E. and Ebrahimi, J., 2014. Generalised transformerless ultra step-up DC–DC converter with reduced voltage stress on semiconductors. *IET Power Electronics*, Vol *7 no* 11, pp.2791-2805, Aug 2014.
8. Zhu, M. and Luo, F.L., 2008. Series SEPIC implementing voltage-lift technique for DC–DC power conversion. *IET Power Electronics*, Vol *1* no1, pp.109-121, Mar 2008.
9. Young, C.M., Chen, M.H., Chang, T.A., Ko, C.C. and Jen, K.K., 2013. Cascade Cockcroft–Walton voltage multiplier applied to transformerless high step-up DC–DC converter. *IEEE transactions on industrial electronics*, Vol *60* no2, pp.523-537, Feb 2017.
10. Sabzali, A.J., Ismail, E.H. and Behbehani, H.M.,. High voltage step-up integrated double Boost–Sepic DC–DC converter for fuel-cell and photovoltaic applications. *Renewable Energy*, Vol *82*, pp.44-53, Oct 2015.
11. Williams, B.W., 2014. Unified synthesis of tapped-inductor dc-to-dc converters. *IEEE Transactions on Power Electronics*, Vol *29 no* 10, pp.5370-5383,Oct 2014.
12. Vazquez, N., Estrada, L., Hernandez, C. and Rodriguez, E.,. The tapped-inductor boost converter. In *Industrial Electronics, 2007. ISIE 2007. IEEE International Symposium on* pp. 538-543. IEEE, June 2007.
13. Zhao, Q. and Lee, F.C., 2003, February. High performance coupled-inductor DC-DC converters. In *Proc. IEEE APEC* Vol. 1, pp. 109-113.
14. Berkovich, Y. and Axelrod, B., Switched-coupled inductor cell for DC–DC converters with very large conversion ratio. *IET power electronics*, vol *4 no* 3, pp.309-315 Oct 2014.
15. Wu, T.F., Lai, Y.S., Hung, J.C. and Chen, Y.M., 2008. Boost converter with coupled inductors and buck–boost type of active clamp. *IEEE Transactions on Industrial Electronics*, Vol *55*no 1, pp.154-162, Jan 2008
16. Zhao, Y., Li, W. and He, X., 2012. Single-phase improved active clamp coupled-inductor-based converter with extended voltage doubler cell. *IEEE transactions on power electronics*, Vol *27* no 6, pp.2869-2878 Jun 2012.
17. Ajami, A., Ardi, H. and Farakhor, A., 2015. A novel high step-up DC/DC converter based on integrating coupled inductor and switched-capacitor techniques for renewable energy applications. *IEEE Transactions on Power Electronics*, Vol *30* no 8, pp.4255-4263 Aug 2015.
18. Tang, Y., Fu, D., Kan, J. and Wang, T., 2016. Dual switches DC/DC converter with three-winding-coupled inductor and charge pump. *IEEE Transactions on Power Electronics*, Vol *31 no* 1, pp.461-469, Jan 2016.
19. Lai, C.M., Pan, C.T. and Cheng, M.C., 2012. High-efficiency modular high step-up interleaved boost converter for DC-microgrid applications. *IEEE Transactions on Industry Applications*, Vol *48 no* 1, pp.161-171 Jan 2012.
20. Tseng, K.C., Huang, C.C. and Shih, W.Y., 2013. A high step-up converter with a voltage multiplier module for a photovoltaic system. *IEEE transactions on power electronics*, Vol *28 no* 6, pp.3047-3057 June 2013.
21. Saravanan, S. and Babu, N.R., 2017. Analysis and implementation of high step-up DC-DC converter for PV based grid application. *Applied Energy*, Vol.*190*, pp.64-72. Mar 2017.
22. Ajami, A., Ardi, H. and Farakhor, A., 2015. A novel high step-up DC/DC converter based on integrating coupled inductor and switched-capacitor techniques for renewable energy applications. *IEEE Transactions on Power Electronics*, Vol *30 no* 8, pp.4255-4263 Aug 2015.
23. Hu, X. and Gong, C., 2014. A high voltage gain DC–DC converter integrating coupled-inductor and diode–capacitor techniques. *IEEE transactions on power electronics*, Vol *29 no* 2, pp.789-800, Feb 2014.
24. Siwakoti, Y.P., Blaabjerg, F. and Loh, P.C., 2016. High Step-Up Trans-Inverse (Tx− 1) DC–DC Converter for the Distributed Generation System. *IEEE Transactions on Industrial Electronics*, Vol *63 no* 7, pp.4278-4291,Jul 2016.
25. Logesh, R., 2017. Resources, configurations, and soft computing techniques for power management and control of PV/wind hybrid system. *Renewable and Sustainable Energy Reviews*, Vol *69*, pp.129-143, Mar 2017.
26. Gandhi, v.., Subramaniyaswamy, v. and Logesh, r., 2017. Topological review and analysis of dc-dc boost converters. *Journal of Engineering Science and Technology*, Vol *12 no* 6, pp.1541-1567, Jun 2017.
27. Kumar, A., Indra, V. and Kumar, S., 2017. Design and implementation of single phase inverter without transformer for PV applications. *IET Renewable Power Generation, Dec 2017*.